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Water Heater Ntc Thermistor Temperature Sensor Probe
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MFP series temperature sensor using the NTC resistance element, according to the different temperature environment or application, through the mature technology, fabricate into a variety of specifications of the sensor, customers can use directly without fabricating.

Technical data
	Item name
	Performance

	Sensing element
	NTC Thermistor various R and B value on request

	Temperature range
	[bookmark: OLE_LINK2][bookmark: OLE_LINK1]-30℃~ +150℃

	Response time
	Water (0.4m/s) T0.63≤30s

	Dissipation factor
	≥2.5mW/℃

	Long-term stability
	Drift≤3% after 1000h heat or cold store (80℃/-30℃

	Dielectric strength
	1500VAC

	Insulation resistance
	≥100MΩ 500VDC



Other options:
1. Standard value:R25℃: 10K  B(25/85℃)=3435K, different NTC R-T performance curve available
2. Different probe and wire length and color available
3. Different size SUS housings available for sensor mounting protection
4. Different type of connector is available




Typical applications:
1. Solar water heater
2. Toilet seat heating
3. Floor heating and cogeneration systems
Features
Moisture-proof, fast response and small time constant etc.
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